Creative TechnologyLasers
180 Alderwood Road      Walnut Creek, CA 94598-1042 USA
925.210.1330 Phone

www.LASER66.com

LASER ENGRAVER SPECIFICATIONS

	L66- 40   SERIES	

	Cut and Engrave 			Parts 	with 	
	CO2 Laser

	Print from Standard 		Computer or with No 		Computer w/ built-			in SD Card Slot

•	up to 1000 dpi resolution and            0.001" repeatability	

•	ASSEMBLED IN USA

•	Optional rotary attachment for round parts 

Engraving Area	20"x12"	
Work Area	20"x12"	
Machine Dimensions	31.5"x20"x8.25"	
Laser Type	Sealed CO2 laser tube	
Net Weight	70 lbs	
Laser Power	40W Peak (30-35W Average)	
Power Supply	AC 110V Native (220V Option Available)	
Gross Power	Less than 1000W	
Driving System	Stepper	
Cooling Mode	Water-cooling and protection system 	
Operating Temperature	0 - 45°C	
Z table	Pat Pend Sliding Z + Removable Floor	
Auxillary Equipment	Exhaust-fans, Air-exhaust pipe	
Controlling Software	Ethernet+USB dual processor ARM+DSP engraving processor, USB Direct Print Drivers (100% USA Software)